# CA LAB TASK: 11

# Muhammad Usman Hussain 12439

# CIRCUIT:

# 

# CODE:

void setup() {

  pinMode(LED\_BUILTIN, OUTPUT);

}

void loop() {

  digitalWrite(LED\_BUILTIN, HIGH);

  delay(1000);

  digitalWrite(LED\_BUILTIN, LOW);

  delay(1000);

}